 نام محصول : دوربین تحت شبکه IP Camera

نوع محصول : Speed dome

سازنده : شرکت فناوری نوین مرصاد فاطر

مدل : SR-1663P-PA

|  |  |  |
| --- | --- | --- |
| **KEY FEACTURE** | | |
| ·Panoramic Camera  ·Four 1/1.8" CMOS  ·Up to  5520x2400@30fps  ·Horizontal: 180°, Verticle:85°  ·Min. illumination Color: 0.0004Lux@F1.0  ·Support region clipping  ·Support distortion correction  ·Detail Camera | | ·Auto-Tracking Early Warning (AEW)  ·Up to  2560\*1440@30fps  ·Optical zoom: 63x, digital zoom 16x  ·Support 3d position  ·Laser Distance: 500m  ·Auto Wiper  ·Built-in Wiper  ·IP66 |
| **Camera** | | |
| **Image Sensor** | Panorama: 1/1.8"   CMOS, Detail: 1/1.8" CMOS | |
| **Signal System** | PAL/NTSC | |
| **Min. Illumination** | Panorama: Color: 0.0004Lux@(F1.0, AGC ON), B/W: 0lux with IR | |
| **Shutter Time** | 1s to 1/100,000s | |
| **Day & Night** | IR Cut Filter with Auto Switch | |
| **Optical Zoom** | Detail: 63x | |
| **Digital Zoom** | Detail: 16x | |
| **Lens** | | |
| **Focal Length** | Panorama: 2.8mm; Detail:   5.7-359mm | |
| **Zoom Speed** | <5s | |
| **Field of View** | Panorama:   Horizontal: 180°,   vertical: 85°  Detail: Horizontal: 60° (w)~1.5° (t), vertical:35° (w)-0.9°(t) | |
| **Aperture Range** | Panorama: F1.0; Detail: F1.6 ~ F5.0 | |
| **Focus Control** | Auto/Manual | |
| **Iris Control** | Auto | |
| **Close Focus Distance** | Detail:1 m–3 m | |
| **Pan & Tilt** | | |
| **Pan Range** | Detail: 0°~360° | |
| **Pan Speed** | Panorama: Pan Manual Speed: 0.1°~200°/s°/s, Pan Preset Speed: 240°/s | |
| **Tilt Range** | Detail: -21°-90° (Auto flip) | |
| **Tilt Speed** | Detail: Pan Manual Speed: 0.1°~120°/s,   Pan Preset Speed: 180°/s | |
| **3D Position** | Yes | |
| **Preset** | 500 | |
| **Preset Accuracy** | ±0.1° | |
| **Cruise** | 16, up to 32 presets per cruise | |
| **Scan** | 8 | |
| **Pattern** | 8, each with 600s memory or 1000 orders | |
| **Scheduled Task** | Preset, Cruise, Scan, Pattern, Alarm output | |
| **Park Action** | Yes | |
| **Power-off Memory** | Yes | |
| **Illuminator** | | | |
| **IR LEDs** | 11 | | |
| **IR Distance** | Up to 300m | | |
| **IR Irradiation Angle** | Adjustable by Zoom | | |
| **White LEDs** | 2, support white/blue/red light flash | | |
| **Laser** | 6, Wavelength 850nm | | |
| **Laser Distance** | Up to 500m | | |
| **IR LEDs** | 11 | | |
| **IR Distance** | Up to 300m | | |
| **Compression Standard** | | | |
| **Video Compression** | S+265/H.265/H.264/M-JPEG | | |
| **Video Bit Rate** | 32Kbps~16Mbps | | |
| **Audio Compression** | G.711A/G.711U/ADPCM\_D/AAC\_LC | | |
| **Audio  Sampling Rate** | 8kHz/32kHz/48kHz | | |
| **Image** | | | |
| **Max. Resolution** | Panorama: 5520x2400;Detail:   2560x1440 | | |
| **Main Stream** | Panorama: PAL:25fps(5520x2400,4096x1800,3840x1680,2784x1200) NTSC:30fps(5520x2400,4096x1800,3840x1680,2784x1200) Detail: PAL:25fps(2560x1440,2304x1296,1920x1080,1280x720) NTSC:30fps(2560x1440,2304x1296,1920x1080,1280x720) | | |
| **Sub Stream** | Panorama: PAL:25fps(2048x896,1280x560,704x320) NTSC:30fps(2048x896,1280x560,704x320) Detail: PAL:25fps(704x576,704x288,352x288,640x360) NTSC:30fps(704X480,704X240,352X240,640x360) | | |
| **Third Stream** | Panorama: PAL:25fps (1280x560) NTSC:30fps (1280x560) Detail: PAL:25fps(704x576,704x288,352x288,640x480) NTSC:30fps(704X480,704X240,352X240,640x480) | | |
| **BLC** | Yes | | |
| **HLC** | Yes | | |
| **WDR** | Panorama :Digital; Detail: 120dB | | |
| **Image Stabilization** | Yes | | |
| **Defog** | Digital | | |
| **White Balance** | Yes | | |
| **AGC** | Yes | | |
| **Noise Reduction** | 2D/3D | | |
| **ROI** | 7 Dynamic Areas for Both Main and Sub Stream | | |
| **Picture Overlay** | Yes | | |
| **Privacy Mask** | Yes | | |
| **Demist** | Yes | | |
| **Image Setting** | Saturation, brightness, contrast, sharpness, adjustable by client software or web browser | | |
| **Flip** | Yes | | |
| **OSD** | Panorama: 16x16, 24x24,32x32,   48x48, 64x64, 96x96, 128x128, adaptable size, letters such as Week, Date, Time, Total 5 Region Detail: 16\*16/24\*24/32\*32/48\*48/64\*64/72\*72/96\*96, adaptable size, letters such as Week, Date, Time, Total 5 Region | | |
| **Feature** | | | |
| **Alarm Trigger** | Event Input, Event Output, Mask   Alarm, Disk Full, Disk R/W Error, IP Address Conflict, MAC Address Conflict, FTP Server Exception | | |
| **Video Analytics** | Panorama: Tripwire, Double Tripwire, Heatmap  Detail: Tripwire, Double Tripwire, Perimeter, Object  Abandon, Object Lost, Loitering, Running, Parking, Heatmap, crowed, People Counting, On Duty Detection, Video Abnormal, Audio Abnormal, Face Capture, Human/Vehicle Classification | | |
| **Early Warning (EW)** | Yes | | |
| **Auto-Tracking** | Yes | | |
| **Face Detection and Analytics** |  | | |
| **Operating Mode** | Face capture, Intelligent monitoring | | |
| **Face Detection Performance** | Detects up to 32 faces at the   same scene | | |
| **Face Exposure Brightness** | Default 35, 1~100 brightness optional | | |
| **Min. Face Pixel** | 29~2560 optional | | |
| **Network** |  | | | |
| **Protocols** | HTTP/HTTPS/TCP/UDP/UPnP/SNMP/DHCP/DNS/DDNS/EasyDDNS/NTP/SMTP/SSL/802.1X/QoS/IPv4/IPv6/PPPOE/Unicast/Multicast/RTMP/RTSP/NFS/FTP | | | |
| **System Compatibility** | ONVIF (PROFILE S/T/G/M), SDK, CGI, P2P | | | |
| **ANR** | Auto store video in SD card when NVR disconnected, and upload video to NVR when resumed connection (Only   Support Sorena ANR NVR) | | | |
| **Remote Connection** | ≤7 | | | |
| **User/Host** | Up to 32 users. 4   user levels | | | |
| **Web** | IE, Firefox, Edge, Safari, Chrome | | | |
| **Interface** | | | | |
| **Communication Interface** | 1 RJ45 100M/1000M  self adaptive Ethernet port | | | |
| **Audio I/O** | 1/1 | | | |
| **Alarm I/O** | 8/2 | | | |
| **Built-In Speaker** | Yes | | | |
| **Reset Button** | Yes | | | |
| **On-board storage** | Built-in Micro SD card slot, up to 512 GB | | | |
| **RS-485** | Yes | | | |
| **BNC** | Yes(Debugging use) | | | |
| **Wiper** | Yes | | | |
| **Electronic Compass** | Yes | | | |
| **GPS/BDS** | N/A | | | |
| **General** | | | | |
| **Protection** | IP66, TVS 6000V lightning   protection, surge protection and voltage transient protection | | | |
| **Operating Conditions** | -40°C~70°C (IR   OFF), -40°C~40°C (IR ON), 0-95%RH | | | |
| **Power Supply** | DC36V±25% | | | |
| **Power Consumption** | 76W MAX | | | |
| **Heater** | Yes | | | |
| **Material** | ADC 12 | | | |
| **Package/Boundary Dimensions** | 565mm(L)\*485mm(W)\*750mm(H) /358mm(L)\*358mm(W)\*568mm(H) | | | |
| **Gross/Net Weight** | 21.7kg (14.8kg) | | | |
| **Protection** | IP66, TVS 6000V lightning   protection, surge protection and voltage transient protection | | | |
| **Web Client Language** | 17 languages Simple Chinese/ Traditional Chinese/ English/ Spanish/ Korean/ Italian/   Turkish/ Russian/ Thai/French/ Polish/ Dutch/ Hebraism/ Arabic/ Vietnamese/   German/ Ukrainian | | | |
| **Operating Conditions** | -40°C~70°C (IR   OFF), -40°C~40°C (IR ON), 0-95%RH | | | |
| **Power Supply** | DC36V±25% | | | |